Overview | Package | Class | Tree | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W X Y

## S

SAT - Static variable in class jcontrol.system.Time
  Weekday code
saveProperties() - Static method in class jcontrol.system.Management
  Saves some properties to the persistent storage.
scale(int, int, int) - Static method in class jcontrol.lang.Math
  Rule of proportion.
scroll(int, int) - Method in class jcontrol.io.Display
  Scrolls the whole display content.
scroll(int, int) - Method in class jcontrol.ui.vole.TextArea
  Scrolls the text.
SCROLL_DOWN - Static variable in class jcontrol.ui.vole.TextArea
  Scroll down
SCROLL_UP - Static variable in class jcontrol.ui.vole.TextArea
  Scroll up
ScrollBar - Class in jcontrol.ui.vole
  This class `ScrollBar` implements a graphical scroll bar.
ScrollBar(int, int, int, boolean) - Constructor for class jcontrol.ui.vole.ScrollBar
  Constructs a new scroll bar.
second - Variable in class jcontrol.system.Time
  The second in the range of 0 to 59.
sectorcount - Variable in class jcontrol.storage.FlashStream
  flash sectorsize and -count
sectorsize - Variable in class jcontrol.storage.FlashStream
  flash sectorsize and -count
seek(int, boolean) - Method in interface jcontrol.io.File
  Sets the read-pointer to a new position.
seek(int, boolean) - Method in class jcontrol.io.Resource
  Sets the read-pointer of this `Resource` to a new position.
select(int) - Method in class jcontrol.ui.vole.ComboBox
  Selects the specified item.
select(int) - Method in class jcontrol.ui.vole.menu.Menu
  Selects the specified menu item.
select(String) - Method in class jcontrol.ui.vole.menu.Menu
  Selects the specified menu item.
select(int) - Method in interface jcontrol.ui.vole.menu.MenuInterface
  Selects the specified menu item.
select(String) - Method in interface jcontrol.ui.vole.menu.MenuInterface
  Selects the specified menu item
selectNextOrPrev(boolean) - Method in class jcontrol.ui.vole.menu.Menu
  Selects the next or previous menu item in this menu.
selectPort(int) - Static method in class jcontrol.comm.RS232Selector
  Select RS232 port
sendACK(byte[]) - Method in class jcontrol.comm.FT1_2
  sends a ACK message (single byte) from within a FT1_2EventListener to generate confirm event
sendRESET() - Method in class jcontrol.comm.FT1_2
  Sends RESET to the BCU and waits for CONFIRM.
sendResponse(byte[]) - Method in class jcontrol.comm.FT1_2
  sends a respond message from within a FT1_2EventListener.
sendUDAT(byte[]) - Method in class jcontrol.comm.FT1_2
  Sends UDAT to the BCU and waits for CONFIRM.
set(int, Object) - Method in class java.util.Vector
  Replaces the element at the specified position in this Vector with the specified element.
setActionListener(ActionListener) - Method in class jcontrol.ui.vole.Button
  Add an ActionListener to the button.
setActionListener(ActionListener) - Method in class jcontrol.ui.vole.CheckBox
  Add an `ActionListener` to the check box.
setActionListener(ActionListener) - Method in class jcontrol.ui.vole.ComboBox
  Sets an `ActionListener` for the `ComboBox`.
setActionListener(ActionListener) - Method in class jcontrol.ui.vole.List
  Sets an `ActionListener` for the `ComboBox`.
setActionListener(ActionListener) - Method in class jcontrol.ui.vole.menu.Menu
  Set the `ActionListener` for this menu.
setActionListener(ActionListener) - Method in class jcontrol.ui.vole.NumberChooser
  Sets an `ActionListener` for the `ComboBox`.
setActionListener(ActionListener) - Method in class jcontrol.ui.vole.RadioButton
  Add an `ActionListener` to the radio button.
setActionListener(ActionListener) - Method in class jcontrol.ui.vole.RockerSwitch
  Add an `ActionListener` to the check box.
setActionListener(ActionListener) - Method in class jcontrol.ui.vole.Slider
  Add an ActionListener to the button.
setActionListener(ActionListener) - Method in class jcontrol.ui.vole.TextArea
  Add an ActionListener to the button.
setActive(int, boolean) - Static method in class jcontrol.io.PWM
  Turns the specified channel on or off.
setAlarm(Time, int) - Static method in class jcontrol.system.RTC
  Sets the alarm time and mode.
setAlign(int, boolean) - Method in class jcontrol.ui.vole.Label
  Set the alignment of the label.
setAnimation(boolean) - Method in class jcontrol.ui.vole.AnimationContainer
  Activate or deactivate the animation of animateable components.
setBackground(int) - Method in class jcontrol.io.Display
  Sets the background color (for text etc.).
setBackground(int) - Method in interface jcontrol.io.Graphics
  Sets the background color (for text etc.).
setBaudrate(int) - Method in class jcontrol.comm.RS232
  Sets the serial port baudrate.
setBeat(int) - Method in class jcontrol.toolkit.iMelody
  Set the beat.
setBounds(int, int, int, int) - Method in class jcontrol.ui.vole.ComboBox
  Set the dimensions of this component.
setBounds(int, int, int, int) - Method in class jcontrol.ui.vole.Component
  Set the dimensions of this component.
setBounds(int, int, int, int) - Method in class jcontrol.ui.vole.graph.Diagram
  Sets a new position and size for the Diagram.
setBounds(int, int, int, int) - Method in class jcontrol.ui.vole.graph.Histogram
  Sets a new position and size for the Histogram.
setBounds(int, int, int, int) - Method in class jcontrol.ui.vole.NumberChooser
  Set the dimensions of this component.
setBrightness(int) - Static method in class jcontrol.io.Backlight
  Set backlight's brightness
setCaption(String, String, int) - Method in class jcontrol.ui.vole.graph.Diagram
  Sets a caption text that is displayed for the min and max value at the left of the diagram.
setCaption(String, String, int) - Method in class jcontrol.ui.vole.graph.Histogram
  Sets a caption text which is displayed for the min and max value at the left of the histogram.
setCaption(String, String) - Method in class jcontrol.ui.vole.meter.AnalogMeter
  Sets a caption text which is displayed for the min and max values at the bottom of the analog meter.
setCaption(String, String) - Method in class jcontrol.ui.vole.meter.BarMeter
  Sets a caption text which is displayed for the min and max value.
setCaption(String) - Method in class jcontrol.ui.vole.meter.FanMeter
  Sets a caption text which is displayed for the min and max values at the bottom of the analog meter.
setCaption(String, String) - Method in class jcontrol.ui.vole.meter.Thermometer
  Sets a caption text which is displayed for the min and max value at the thermometer.
setClassPersistence(boolean) - Static method in class jcontrol.system.Management
  Marks the calling class not to be removed from the garbage collector.
setColor(int) - Method in class jcontrol.io.Display
  Sets the foreground color.
setColor(int) - Method in interface jcontrol.io.Graphics
  Sets the foreground color.
setCycles(int, int) - Static method in class jcontrol.io.PWM
  Sets both the prescale and the preload value of the PWM unit.
setDaemon(boolean) - Method in class java.lang.Thread
  Marks this thread as either a daemon thread or a user thread.
setDisplayMode(int) - Method in class jcontrol.io.Display
  Sets the displaymode.
setDrawMode(int) - Method in class jcontrol.io.Display
  Sets the drawing mode.
setDrawMode(int) - Method in interface jcontrol.io.Graphics
  Sets the drawing mode.
setDuty(int, int) - Static method in class jcontrol.io.PWM
  Sets the duty cycle of the given channel.
setErr(ConsoleOutputStream) - Static method in class java.lang.System
  Reassigns the "standard" error output stream.
setFocus(Component) - Method in class jcontrol.ui.vole.Container
  Set the focus to the given component.
setFont(Object) - Method in class jcontrol.io.Display
  Sets the font to use.
setFont(Object) - Method in interface jcontrol.io.Graphics
  Sets the font to use.
setFont(Resource) - Method in class jcontrol.ui.vole.Component
  Sets the font for this component.
setFont(Resource) - Method in class jcontrol.ui.vole.Container
  Set the font for this component.
setFont(Resource) - Method in class jcontrol.ui.vole.menu.Menu
  Set the font for this component.
setFont(Resource) - Method in class jcontrol.ui.vole.NumberChooser
  Sets the font for this component.
setFrequency(int) - Static method in class jcontrol.io.PWM
  Sets the frequency of the PWM signal (in Hz), uses `setCycles()`.
setFrequency(byte, int) - Static method in class jcontrol.io.PWMext
  Sets the frequency of the PWM signal (in Hz), of the given channel.
setGraphics(Graphics) - Method in class jcontrol.ui.vole.Component
  This method is called to set the main Display context for this component.
setGraphics(Graphics) - Method in class jcontrol.ui.vole.Container
  Sets the Display context for all child components.
setGraphics(Graphics) - Method in interface jcontrol.ui.vole.menu.MenuInterface
  This method is called to set the main Display context for this component.
setIn(ConsoleInputStream) - Static method in class java.lang.System
  Reassigns the "standard" input stream.
setInterval(int) - Method in class jcontrol.ui.vole.AnimationContainer
  Set the interval between two animation steps.
setLabel(String) - Method in class jcontrol.ui.vole.Border
  Sets the label of this border.
setLabel(Object) - Method in class jcontrol.ui.vole.Button
  Change the button's label
setLabel(String) - Method in class jcontrol.ui.vole.CheckBox
  Change the label if this check box.
setLabel(Object, boolean) - Method in class jcontrol.ui.vole.Label
  Set a new label to display.
setLabel(String) - Method in class jcontrol.ui.vole.RadioButton
  Change the label if this radio button.
setListener(FT1_2EventListener) - Method in class jcontrol.comm.FT1_2
  sets a FT1_2EventListener
setLock(Object, boolean) - Static method in class jcontrol.system.Management
  Locks or unlocks an object in memory.
setMenu(MenuInterface) - Method in class jcontrol.ui.vole.Frame
  Add a menu to this frame.
setMenu(MenuInterface) - Method in class jcontrol.ui.vole.PassiveFrame
  Add a menu to this frame.
setMode(int, int) - Static method in class jcontrol.io.GPIO
  Sets the mode of the given pin.
setNotes(String) - Method in class jcontrol.toolkit.iMelody
  Set the melody string.
setNumericDisplay(int, int, String) - Method in class jcontrol.ui.vole.meter.AnalogMeter
  Sets the parameters of the numeric value display.
setNumericDisplay(int, int, String) - Method in class jcontrol.ui.vole.meter.BarMeter
  Sets the parameters of the numeric value display.
setNumericDisplay(int, int, String) - Method in class jcontrol.ui.vole.meter.FanMeter
  Sets the parameters of the numeric value display.
setNumericDisplay(int, int, String) - Method in class jcontrol.ui.vole.meter.Thermometer
  Sets the parameters of the numeric value display.
setOut(ConsoleOutputStream) - Static method in class java.lang.System
  Reassigns the "standard" output stream.
setParams(int) - Method in class jcontrol.comm.RS232
  Sets some serial port feature parameters.
setParent(Container) - Method in class jcontrol.ui.vole.Component
  Sets the parent Container
setParent(Container) - Method in class jcontrol.ui.vole.menu.Menu
  Sets the parent Container.
setParent(Container) - Method in interface jcontrol.ui.vole.menu.MenuInterface
  Sets the parent Frame.
setPeriod(int) - Static method in class jcontrol.io.PWMext
  Sets the period of the PWM signal (in microseconds).
setPeriod(byte, int) - Static method in class jcontrol.io.PWMext
  Sets the period of the PWM signal (in microseconds) of the given channel.
setPixel(int, int) - Method in class jcontrol.io.Display
  Sets a single pixel on the display to foreground color.
setPixel(int, int) - Method in interface jcontrol.io.Graphics
  Sets a single pixel on the graphics device to foreground color.
setPriority(int) - Method in class java.lang.Thread
  Changes the priority of this thread.
setProperty(String, String) - Static method in class jcontrol.system.Management
  Sets the JControl system Property to the specified value.
setRadioButton(RadioButton) - Method in class jcontrol.ui.vole.Container
  Set the state of the radio buttons contained in this `Container`.
setScrollPos(int) - Method in class jcontrol.ui.vole.TextArea
  Sets the absolute scroll position of the text area.
setSize(int) - Method in class java.util.Vector
  Sets the size of this vector.
setState(int, boolean) - Static method in class jcontrol.io.GPIO
  Sets a single IO-Pin.
setState(boolean) - Method in class jcontrol.ui.vole.CheckBox
  Set the state of this `CheckBox`.
setState(boolean) - Method in class jcontrol.ui.vole.RadioButton
  Set the state of this `RadioButton` to "on" (true) or "off" (false).
setState(boolean) - Method in class jcontrol.ui.vole.RockerSwitch
  Set the state of this `RockerSwitch`.
setStep(int) - Method in class jcontrol.ui.vole.TextScroller
  Sets the step width of this text scroller in pixels.
setStyle(int) - Method in class jcontrol.toolkit.iMelody
  Set the music style.
setStyle(int) - Method in class jcontrol.ui.vole.Border
  Sets the style of this border.
setTime(Time) - Static method in class jcontrol.system.RTC
  Sets the current time.
setValue(int) - Method in class jcontrol.ui.vole.graph.Diagram
  Adds a new value to the Diagram.
setValue(int) - Method in class jcontrol.ui.vole.graph.Histogram
  Adds a new value to the Histogram.
setValue(int, int, int) - Method in class jcontrol.ui.vole.meter.AnalogClock
  Sets a the specified time to the clock.
setValue(int) - Method in class jcontrol.ui.vole.meter.AnalogMeter
  Sets the current analog meter value.
setValue(int) - Method in class jcontrol.ui.vole.meter.BarMeter
  Sets the bar graph value.
setValue(int) - Method in class jcontrol.ui.vole.meter.DigitalMeter
  Sets the value to display on the LCDMeter.
setValue(int) - Method in class jcontrol.ui.vole.meter.FanMeter
  Sets the fans value.
setValue(int) - Method in class jcontrol.ui.vole.meter.SevenSegmentMeter
  Sets the value to display on the SevenSegmentMeter.
setValue(int) - Method in class jcontrol.ui.vole.meter.Thermometer
  Sets the thermometer value.
setValue(int) - Method in class jcontrol.ui.vole.NumberChooser
  Sets the specified value.
setValue(int) - Method in class jcontrol.ui.vole.ScrollBar
  Sets a new scroll value in percent and repaints the scrollbar.
setValue(int) - Method in class jcontrol.ui.vole.Slider
  Set the slider value.
setVisible(boolean) - Method in class jcontrol.ui.vole.Component
  Turns the component visible or invisible.
setVisible(boolean) - Method in class jcontrol.ui.vole.Container
  Sets this container and all child comonents visible or invisible.
setVisible(boolean) - Method in class jcontrol.ui.vole.Frame
  Shows or hides the frame.
setVisible(boolean) - Method in class jcontrol.ui.vole.PassiveFrame
  Shows or hides the frame.
SevenSegmentMeter - Class in jcontrol.ui.vole.meter
  This class `SevenSegmentMeter.class` provides a seven-segment-based lcd-style counter with a variable number of digits.
SevenSegmentMeter(int, int, int, int, int, int) - Constructor for class jcontrol.ui.vole.meter.SevenSegmentMeter
  Creates a new SevenSegmentMeter.
show() - Method in class jcontrol.ui.vole.Frame
  Shows the frame.
show() - Method in class jcontrol.ui.vole.PassiveFrame
  Shows the frame.
SIMPLE_BORDER - Static variable in class jcontrol.ui.vole.Border
  Simple rectangular border
sin(int) - Static method in class jcontrol.lang.Math
  Look-up table sine function.
size() - Method in class java.util.Vector
  Returns the number of components in this vector.
sleep(int) - Static method in class jcontrol.lang.ThreadExt
  Causes the currently executing thread to sleep (temporarily cease execution) for the specified number of milliseconds.
Slider - Class in jcontrol.ui.vole
  This is a graphical slider for JControl.
Slider(int, int, int, int, int) - Constructor for class jcontrol.ui.vole.Slider
  Constructs a slider and sets bounds.
Slider(int, int, int, int, int, int) - Constructor for class jcontrol.ui.vole.Slider
  Constructs a slider and sets bounds.
SoundDevice - Interface in jcontrol.io
  Defines behaviour for any single voice noise making device.
source - Variable in class jcontrol.ui.vole.event.ActionEvent
sqrt(int) - Static method in class jcontrol.lang.Math
  Look-up table square root.
STACC - Static variable in class jcontrol.toolkit.iMelody
  Staccato mode
start() - Method in class java.lang.Thread
  Causes this thread to begin execution; the Java Virtual Machine calls the `run` method of this thread.
start(String, String[], boolean) - Static method in class jcontrol.system.Management
  Starts a Java application.
STATE_CHANGED - Static variable in class jcontrol.ui.vole.event.ActionEvent
  An component's state was changed
STD_LF - Static variable in interface jcontrol.comm.ConsoleOutputStream
  The standard linefeed character to print.
stop() - Method in class jcontrol.toolkit.iMelody
  Stops the music playing.
String - Class in java.lang
  The `String` class represents character strings.
String() - Constructor for class java.lang.String
  Initializes a newly created `String` object so that it represents an empty character sequence.
String(byte[]) - Constructor for class java.lang.String
  Construct a new `String` by converting the specified array of bytes using the platform's default character encoding.
String(byte[], int, int) - Constructor for class java.lang.String
  Construct a new `String` by converting the specified subarray of bytes using the platform's default character encoding.
substring(int, int) - Method in class java.lang.String
  Returns a new string that is a substring of this string.
SUN - Static variable in class jcontrol.system.Time
  Weekday code
switchBank() - Static method in class jcontrol.system.Management
  Switches the flash bank to the bank specified by property ``system.userbank``.
System - Class in java.lang
  The `System` class contains several useful class fields and methods.
System() - Constructor for class java.lang.System
SYSTEMFONT - Static variable in class jcontrol.io.Display
  Used to specify the internal font with `Display.setFont(Object)`.

Overview | Package | Class | Tree | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W X Y