Overview | Package | Class | Tree | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W X Y

## F

FanMeter - Class in jcontrol.ui.vole.meter
  This class `FanMeter`implements a simple animation representing a fan.
FanMeter(int, int) - Constructor for class jcontrol.ui.vole.meter.FanMeter
  Create a FanMeter with the specified label and coordinates.
File - Interface in jcontrol.io
  Provides a set of methods for file-system access.
FILL_LINE - Static variable in class jcontrol.ui.vole.meter.BarMeter
  Line style
FILL_SOLID - Static variable in class jcontrol.ui.vole.meter.BarMeter
  Solid style
fillRect(int, int, int, int) - Method in class jcontrol.io.Display
  Draws a filled rectangle.
fillRect(int, int, int, int) - Method in interface jcontrol.io.Graphics
  Draws a filled rectangle.
findNext(TlvFile, byte) - Method in class jcontrol.storage.FlashTlv
  Finds the next file with the specified tag.
findNext(TlvFile) - Method in class jcontrol.storage.FlashTlv
  Finds the next file.
firstElement() - Method in class java.util.Vector
  Returns the first component (the item at index 0) of this vector.
Flash - Class in jcontrol.io
  Raw access to JControls flash memory.
Flash() - Constructor for class jcontrol.io.Flash
  Constructs a `Flash`-Object with access to the default bank (of the current application), is equivalent to `Flash(-1)`.
Flash(int) - Constructor for class jcontrol.io.Flash
  Constructs a Flash-Object to a specific bank.
FLASHACCESS - Static variable in class jcontrol.io.Resource
  Constructor parameter for access to the external flash memory.
FlashStream - Class in jcontrol.storage
  This class `FlashStream` represents a memory cached data stream for reading and writing continuous data to the flash memory.
FlashStream() - Constructor for class jcontrol.storage.FlashStream
  Create a new flash stream.
FlashTlv - Class in jcontrol.storage
  This class `FlashTlv.class` implements a tag-length-value file system.
FlashTlv(int) - Constructor for class jcontrol.storage.FlashTlv
  Creates a new FlashTlv object.
FLOATING - Static variable in class jcontrol.io.GPIO
  Represents a floating GPIO input mode.
FLOWCONTROL_RTSCTS - Static variable in class jcontrol.comm.RS232
  Enables hardware handshaking using `RTS` and `CTS` lines.
FLOWCONTROL_XONXOFF - Static variable in class jcontrol.comm.RS232
  Enables software handshaking using `XON` and `XOFF` symbols.
focusOwner - Static variable in class jcontrol.ui.vole.Component
  Current focus owner (global flag)
font - Variable in class jcontrol.ui.vole.Component
  A font resource for drawing text.
format(int) - Method in class jcontrol.storage.FlashTlv
  Formats the available flash.
Frame - Class in jcontrol.ui.vole
  A Frame is the starting point for creating a graphical user interface.
Frame() - Constructor for class jcontrol.ui.vole.Frame
  Constructs a new Frame.
Frame(Graphics, Keyboard) - Constructor for class jcontrol.ui.vole.Frame
  Constructs a new Frame.
FRI - Static variable in class jcontrol.system.Time
  Weekday code
FT1_2 - Class in jcontrol.comm
  Partial implementation of the FT1.2 protocol.
FT1_2() - Constructor for class jcontrol.comm.FT1_2
  Constructs a new FT1_2 instance using the serial line.
FT1_2EventListener - Interface in jcontrol.comm
  Registered implementers are called from within the `FT1_2` event loop, you have to reply for complete transmisstions.

Overview | Package | Class | Tree | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P R S T U V W X Y